# 2-port Parameter block

This component inserts a 2-port block. The 2-port can be another 2-port schematic, or a file that is read from disk.

For a file that is read from disk, each line in the file must have the following format:

> freq mag(P11) ang(P11) mag(P21) ang(P21) mag(P12) ang(P12) mag(P22) ang(P22)

The parameters can by in S,Y or Z parameter format. The type is determined by the file extension (s2p, y2p or z2p). For S parameter data the normalising impedance is assumed to be 50 ohms and all angles should be in degrees.

Model:

Parameters:

> Name: This must be the name of schematic or file.

ViPEC Development team (vipec-developers@lists.sourceforge.net)